УДК: 53.043, 532.5, 533.6.01, 533.16, 533.17

PACS: 47.10.-g, 47.32.-y

DOI:

Full name: Vadym Alexeevich Ostanin

Self employed engineer

**Repulsion and attraction between spinning cylinders in viscous fluids**

**V.A. Ostanin**

03039, 16 Demiivska Str, Kyiv, Ukraine

**Abstract**

**Purpose.** The effects ofcontrollable attraction and repulsion of spinning circular object in an incompressible viscous fluid is proposed. This study provides an overview and numerical simulation of the push/pull effects caused by pair of spinning discs. The purpose of this study is to explain principles that cause push/pull effects pair of spinning circular objects in the fluid medium and investigate dependencies of force on relative spin directions and rotation speed. Repulsion and attraction fluid effects can be used as a method of controllable touchless interaction without magnetic field. This study was inspired by magnetic effects caused by "spin" property of electrons and push/pull effects between two current-carrying wires.

**Methods.** The practical experiment uses a pair of plastic tubes that driven by motors and spin close to each other in air at an atmospheric pressure. Numerical simulation helps to predict amount of force that produced by rotating cylinders.

**Results.** A spinning disc adjacent to another spinning disc forms space of high or low pressure of air between them depending on spin direction. Spinning neighbored discs with opposite spin directions leads to helps neighbored flow to keep air circulation in gap that reduce air pressure between spinning objects and attracts them. Vise-versa, spinning discs with same directions damp and squash air flow in gap that increase air pressure between spinning objects that repel them. Dependency between directions of spinning objects and observed ​effects had been verified by numerical simulation using software OpenFOAM version 9.

**Conclusions.** Observed repulsion and attractioneffects can be exploited to manipulate objects in cases where magnetic or other touchless interactions aren’t possible. Also, it can be used as analogy to magnetic repulsion and attractioneffects between two current-carrying wires.

1. **Introduction.**

This article describes the experiment of controlled attraction and repulsion in a viscous air medium and provides a numerical simulation of the observed effects in an incompressible fluid viscous laminar vortex-free medium of gas and liquid with Reynolds number from 50×10^3 for air, and up to 724×10^3 for water between two spinning discs. This effect is useful for the engineering task of non-contact interaction between objects, when electric or magnetic fields can adversely affect the engineering task. The described effect was discovered under inspiration from the study of magnetic effects caused by the “spin” property of an electron in conductors with current, but, as will be shown in the article, similar effects are observed in fluid media. These effects are described initially in the article [1]. The object of the study is two plastic cylinders 10 cm long and 5 cm in diameter, driven by engines. The subject of the study is the attraction and repulsion effects that occur between rotating cylinders, and it is also studied how the effects depend on the interactions of fluid circulations around the cylinders. Combining or colliding circulation leads to an increase or decrease in pressure in the space between the cylinders, respectively. A practical experiment was carried out in an air stationary viscous medium at atmospheric pressure. For a visual explanation of the effects, the results of numerical simulations for air and water at a cylinder speed of 10^4 RPM are given.

1. **Methods**

The experimental equipment (**Fig. 1.**) consists of two smooth plastic cylinders 50 mm in diameter and 100 mm long. They are driven by two independent motors powered by a direct current source. One of the cylinders is suspended on a thin wire to the frame, and the second is in a free position for manipulating it by hand. Wire was used in place of thread to reduce untwisting due to the untwisting properties of thread under tension. Around the installation, the air is 25 ̊ stationary with atmospheric pressure. With both motors turned on, the cylinders spin up to a stable speed of approximately 10^4 RPM. The rotation speed was measured with a digital tachometer with an accuracy of 0.05%.



**Fig. 1.** Rotating cylinder geometry

Initial data:

- cylinder radius

– cylinder angular velocity

– air density at 25 ̊

*–* kinematic viscosity of air at 25 ̊

*–* dynamic viscosity of air at 25 ̊ =

– water density at 25 ̊

*–* kinematic viscosity of water at 25 ̊

*–* dynamic viscosity of water at 25 ̊ =

By giving each cylinder (**Fig. 2.**) a rotation, a boundary layer will form on the rotating body of revolution due to the sticking condition to the body surface with the effect of “no-slip condition”, which means that at the boundary of a solid object, a viscous fluid flows with zero velocity relative to this border (**Fig. 3.**). As each cylinder rotates, this creates a very thin "boundary layer" around the cylinder, the air next to the cylinder simply rotates with it at the same speed (**Fig. 4.**). The cylinder literally drags air along with it. And in the next layers, rotation in a viscous medium creates an irrotational circulation of the flow in a circle around the cylinder.



**Fig. 2.** Rotating cylinder geometry

**Fig. 4.** Circulation around cylinder

**Fig. 3.** Boundary layer flow over a rotating disc [2].

Initially, under the given experimental conditions, the cylinders rotated in opposite directions, then the manual cylinder was brought up to the hanging cylinder. At the same time, the attraction of the hanging cylinder to the hand one at a distance of 5 or less centimeters were observed. By changing the experimental conditions and rotating the cylinders in one direction, the hand cylinder was also brought up to the hanging cylinder, and at a distance of 5 or less centimeters, the hanging cylinder was observed to repulse the hand cylinder.

To confirm the causes of the observed effects, OpenFOAM version 9 numerical simulation software with a PISO solver was used. The model includes the calculation of turbulent flows using the Large Eddy Simulation method. The calculation results and graphs are shown after running the simulation for 40 seconds. The results for 4 simulations are presented in the article. The difference between the simulations is presented in the table (**Table 1.**)

|  |  |  |
| --- | --- | --- |
| Simulation name | Spin direction of one of the cylinders (0.orig/U) | transportProperties |
| Attraction in air | code  #{  …  rot = -10000.0/60\*6.28\*vector(0,0,1)^(Cf-vector(0.075,0.0, 0.0));  operator==(rot);  #}; | transportModel Newtonian;  nu nu [ 0 2 -1 0 0 0 0 ] 1.56e-05;  rho rho [ 1 -3 0 0 0 0 0 ] 1.185; |
| Repulsion in air | code  #{  …  rot = 10000.0/60\*6.28\*vector(0,0,1)^(Cf-vector(0.075,0.0, 0.0));  operator==(rot);  #}; | transportModel Newtonian;  nu nu [ 0 2 -1 0 0 0 0 ] 1.56e-05;  rho rho [ 1 -3 0 0 0 0 0 ] 1.185; |
| Attraction in water | code  #{  …  rot = -10000.0/60\*6.28\*vector(0,0,1)^(Cf-vector(0.075,0.0, 0.0));  operator==(rot);  #}; | transportModel Newtonian;  nu nu [ 0 2 -1 0 0 0 0 ] 0.903e-06;  rho rho [ 1 -3 0 0 0 0 0 ] 997.3; |

|  |  |  |
| --- | --- | --- |
| Repulsion in water | code  #{  …  rot = 10000.0/60\*6.28\*vector(0,0,1)^(Cf-vector(0.075,0.0, 0.0));  operator==(rot);  #}; | transportModel Newtonian;  nu nu [ 0 2 -1 0 0 0 0 ] 0.903e-06;  rho rho [ 1 -3 0 0 0 0 0 ] 997.3; |

1. **Results**
   1. **One cylinder**

As the speed of the boundary layers increases the viscous air flow around the cylinder, forming separate irrotational circulations of air flows in the form of concentric circles (**Fig. 5.**). With a sharp start of the rotation of the cylinder, vortex flows can first be observed, but after a few seconds, the circulation becomes without vortex. Viscous friction significantly affects the behavior of the medium. The circulation of fluid flows, due to the forces of viscous friction, occurs around a rotating cylinder. In the boundary zone of air and cylinder, the pressure is the lowest due to the high flow velocity (**Eq. 1.**), which is consistent with the Bernoulli equation for viscous fluids:

|  |  |
| --- | --- |
|  | (1) |



**Fig.** 5**.** Single cylinder circulation simulation with RPM

The fluid circulation rate around the cylinder is inversely proportional to the distance from the cylinder (**Eq. 2.**)(**Fig. 6.**).

|  |  |
| --- | --- |
|  | (2) |



**Fig. 6.** Single cylinder velocity distribution in meters, RPM

When rotating, the cylinder entrains adjacent layers of air, causing it to circulate. Irrotational circulations of a viscous medium cover the entire space outside the cylinder, provided that the space around is boundless. But if the space is limited, for example by walls, then vortices appear in the region of the walls. But the flow velocity in these swirls is much less than the main flow near the cylinder, so they are not considered in the observations of the effects. The greater the viscous friction, the more stable the circulations, and the slower the circulation speed decreases, moving away from the cylinder. The fluid flow velocity is different near the walls and away from them. If we introduce a transverse (perpendicular to the velocity vector) coordinate of the distance from the surface of the cylinder r, then the fluid velocity is a function of this distance v(r) (**Fig. 6.**). This dependence is determined by the momentum transfer in the transverse direction or otherwise by the velocity gradient, as in the case of a viscous gas:

|  |  |
| --- | --- |
|  | (3) |

Force of interaction of adjacent layers touching on the surface :

|  |  |
| --- | --- |
|  | (4) |

Moving away from the cylinders, the circulation rate decreases, keeping the pressure close to stationary, which is higher relative to the vicinity of the cylinder (**Fig. 7.**).



**Fig. 7.** Data representation of the kinematic pressure of simulation

**3.2. Fluid attraction effect**

For numerical simulation near the surface of the cylinder, where higher accuracy is required, a fine mesh is used. Moving away from the surface, the mesh becomes coarser (**Fig. 8.**).

****

**Fig. 8**. Computational grid.

Два цилиндра диаметром 0.05 метра на расстоянии 0.025 метра друг от друга настраиваются на вращение в противоположных направлениях, например один цилиндр настраивается на вращение против часовой стрелки, а другой по часовой стрелке. Между цилиндрами потоки сходятся, сохраняя высокую скорость циркуляции, и понижая давление между ними (**Fig. 9.**). Скорость циркуляции каждого цилиндра между цилиндрами не уменьшается с ростом расстояния, а она поддерживает скорость за счёт циркуляции соседнего цилиндра (**Fig. 10.**). Разность давлений снаружи цилиндров и внутри цилиндров создаёт силу, действующую на каждый цилиндр в отдельности, направленную снаружи каждого цилиндра во внутрь пространства между цилиндрами (**Fig. 11.**).



**Fig. 10.** Air flow velocity distribution view of simulation

**Fig. 9.** Air flow circulation stream tracer of simulation



b)

**Fig. 11.** Air pressure distribution view of simulation.

Сила, возникающая из-за разности внешнего и внутреннего давления, вычисляется с помощью формулы из определения давления:

|  |  |
| --- | --- |
|  | (5) |

Тогда сила равна произведению разности давлений на площадь поверхности испытующей давление:

|  |  |
| --- | --- |
|  | (6) |

Из результатов симуляции (**Fig. 12.**) видно, что давление между цилиндрами посередине равно

|  |  |
| --- | --- |
| . | (7) |

 

b)

a)

**Fig. 12.** Data representation of simulation:

a) Air velocity; b) Kinematic pressure

Если задать давление вне цилиндров атмосферное стационарное как , где скорость флюидов мизерна по сравнению со скоростью самого цилиндра, то разность давлений (**Eq. 5.**) относительно атмосферного равна:

|  |  |
| --- | --- |
|  | (8) |

Площадь контакта внешнего давления по направлению в пространство между цилиндрами равна половине поверхности цилиндра:

|  |  |
| --- | --- |
|  | (9) |
|  | (10) |

Используя разность давлений (**Eq. 6.**) и площадь контакта (**Eq. 9.**), сила (**Eq. 6.**) вычисляется как:

|  |  |
| --- | --- |
|  | (11) |

Используя формулы выше (**Eq. 5, 9.**), вычислим силу . Для этого зададим для воды также как и для воздуха, потому что внешнее давление равно стационарному давлению. Внутреннее давление между цилиндрами дано из графика распределения давлений (**Fig. 13.**).

|  |  |  |
| --- | --- | --- |
|  | | (12) |
|  | | (13) |
|  | (14) |

Используя разность давлений и площадь контакта , сила вычисляется как:

|  |  |
| --- | --- |
|  | (15) |

**

**Fig. 13.** Water kinematic pressure distribution graph of simulation.

**3.3. Эффект флюидного отталкивания**

Оба цилиндра настраиваются на вращение в одинаковых направлениях, например один цилиндр настраивается на вращение против часовой стрелки, а другой по часовой. По мере увеличения скорости их пограничные слои ускоряют поток воздуха вокруг каждого из них формируя отдельные потоки воздуха в виде концентрических окружностей. Поднося цилиндры ближе по мере увеличения скорости пограничного слоя, потоки воздуха вокруг цилиндров объединяются, формируя единый поток (**Fig. 14.**). Но не весь поток движется ламинарно вокруг цилиндров.

Потоки воздуха у пограничного слоя цилиндра, придавленные внешним атмосферным давлением, всё ещё пытаются двигаться вокруг каждого из цилиндров. Но пытаясь двигаться между цилиндрами, встречают встречный поток от соседнего цилиндра.



**Fig. 14.** Air flow circulation using stream tracer of simulation

Это столкновение потоков останавливает циркуляцию в центре, а создаёт избыточное давление между цилиндрами (**Fig. 15.**). Это избыточное давление больше атмосферного и благодаря ему оба цилиндра стремятся оттолкнуться от зоны между цилиндрами. Также, из-за столкновения встречных циркуляционных потоков, скорость потоков между цилиндра практически равна нулю (**Fig. 16.**).



**Fig. 15.** Air pressure distribution view of simulation.



**Fig. 16.** Air flow velocity view

Используя формулы приведенные выше (**Eq. 5, 6, 9, 10.**) и данные из графика (**Fig. 17.**) и можно посчитать силу отталкивания:

|  |  |
| --- | --- |
| . | (16) |
|  | (17) |
|  | (18) |
| . | (19) |
|  | (20) |
|  | (21) |

****

**Fig. 17.** Kinematic pressure distribution:

a) Air; b) Water

**4. Выводы**

Эффекты притяжения и отталкивания между двумя вращающимися цилиндрами в несжимаемой вязкой жидкости численно исследуется для воздуха и водных жидкостей с использованием программного обеспечения OpenFOAM 9 с использованием решателя PISO. Скорость вращения устанавливается фиксированной , что соответствует числам Рейнольдса для воздуха, и для воды. Результаты полученные с помощью численных методов подтверждают наличие разности давлений, вызывающие эффекты притяжения и отталкивания в флюидной среде двух и более вращающихся цилиндров. Эта работа показала, что в воде по сравнению с воздухом эффекты более выраженны. При решении инженерных задач бескотактного и безмагнитного взамодействия, водная среда подходит больше из-за большей динамической вязкости и большей силы оказываемого действия эффектами.

REFERENCES

1. **Title:** On the Attraction between Two Rotating Parallel Cylinders in Some Viscous Liquids  
   **Authors:** Nukiyama, D.  
   **Journal:** Japanese Journal of Astronomy and Geophysics, Vol. 2, p.193-207  
   **Bibliographic Code:** 1925JaJAG...2..193N
2. Бутиков Е.И. Физика Кн.1 страницы 348-349;
3. Peter R.N. Childs. Rotating Flow, DOI: 10.1016/B978-0-12-382098-3.00006-8, Chapter 6
4. Р. Фейнман, Р. Лейтон, М. Сэндс. Фейнмановские лекции по физике. Том 2. Электромагнетизм и материя, § 4. Циркуляция, § 1. Вязкость, § 2. Вязкий поток
5. Г. Биркгоф “Гидродинамика”, 1960, страницы 32-33.
6. В.А. Бударин “Метод расчёта движения жидкости”, 2006,страницы 31-38, 98.
7. Б.Н. Юрьев “Экспериментальная аеродинамика” “Часть 1” “Теоретические основы экспериментальной аеродинамики”, 1939, страницы 96-113